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Abstract 
Among the alloys, the most used in additive manufacturing (AM) technologies are surely Co-Cr, Ti-, Al- and Ni-alloys. Such alloys cover the most widespread industrial applications form automotive/aerospace, to medical, energy and Oil&Gas. The material qualification process of the alloys in the specific environment is nowadays gaining lot of importance, as the corrosion behavior of traditional casting and wrought alloys is well known, but it significantly modifies due to macro and microstructure modifications induced by additive manufacturing process (Fig. 1). The results of several reserches emphasize strict correlation between the corrosion behavior and the unique microstructure of these alloys, thus giving rise to new opportunities for increasing the knowlwge in corrosion science. Corrosion mechanisms are also affected by both the production processes and heat treatments (Fig.2). Additive technologies have several and undubtful advantages compared to subtractive ones, mainly due to the possibility to produce components with very complex and non-dense geometries (micro and macro porous, trabecular, etc.). The unique microstructure, the widening of the solubility field of the alloy elements due to rapid cooling, the precipitation of non-equilibrium phases, the different surface conditions and heat treatments are only some of the elements affecting both the mechanical behaviour and the corrosion resistance. In fact, for applications in particularly aggressive environments, the qualification of these materials must be completely re-discussed, as well as the definition of new production standards and post-processing heat treatments specifically designed to enhance their peculiarities. 
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	Fig.1:  Schematic representation of the microstrucutre of the alloy AlSi10Mg obtained by means laser powder bed fusion as a function of the directions of the production (Cabrini et al., J. Mat. Proc. Tech. 231 (2016) 326–335 
	Fig. 2: effect of the temperature of post processing heat treatments on the corrosion behavior of the AlSi10Mg alloy (Cabrini et al., Materials 2018, 11, 1051 
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