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Abstract 
Hydrogen is an energy carrier, which holds tremendous promise as a new clean energy option. Hydrogen storage, which is considered to be the most important factor cutting across both hydrogen production and hydrogen transportations, has been the subject of intensive research for many years. Mg and Mg-based materials have opened promising concept for storing hydrogen in a solid-state matter. The natural abundance, cheap price, operational cost effectiveness, light weight, and high hydrogen storage capacity (7.60 wt.%, 0.11 kg H2L−1) are some advantages of Mg and Mg-based alloys making them desirable storage materials for research and development. Whereas all catalytic materials used to improve the behaviors of hydrogenation/dehydrogenation kinetics for MgH2 have long-range order structure, the present work proposes two different types of structure; i.e. short range- and medium range- order. 
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Fig. HRTEM images of nanocrystalline MgH2 powders doped with 10 wt.% of (a) amorphous Zr2Ni, and (b) big-cube Zr2Ni nanopowders. The corresponding illustration sketches for the HRTEM images shown in (a) and (b) are displayed in (c) and (d), respectively.
For the purpose of the present study, MgH2 powders were prepared by reactive ball milling of Mg powders under 50 bar of H2, using room-temperature high-energy ball mill [5]. Ultrafine powders of amorphous- and big cube-Zr2Ni phases were prepared by ball milling small bulk pieces of tetragonal-Zr2Ni alloy prepared by arc melting technique. Small volume fraction (10 wt. %) of amorphous and big-cube powders obtained after ball milling for 100 and 150 h, respectively were individually mixed with as-synthesized MgH2 powders and then ball milled for 50 h. 

The results have shown that nanocomposite MgH2/10 wt.% metallic glassy Zr2Ni powders had high density of hydrogen (∼6 wt.%) and possessed fast kinetics of hydrogen uptake/release at 250 °C within 1.15 and 2.5 min, respectively. Whereas, MgH2/10 wt.% of big cube Zr2Ni nanocomposite showed moderate improvement on hydrogenation (1.8 min)/dehydrogenation (7 min) kinetics due to the heterogeneous distribution of their particles onto the MgH2 powders. 
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