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The application of the electromagnetoelastic actuator based on the electromagnetoelasticity for the piezoelectric, piezomagnetic, electrostriction, magnetostriction effects is promising in the nanotechnology, the nanobiology, the power engineering, the microelectronics, the adaptive optics equipment. The correcting devices are chosen for providing the high quality of the control systems for the deformation of the piezoactuator. The analytical expressions for the sufficient absolute stability conditions of the system with the hysteresis nonlinearity of the electromagnetoelastic actuators are written using the Yakubovich absolute stability criterion with the condition on the derivative, which is the development of the Popov absolute stability criterion. For the Lyapunov-stable control system, the Yalubovich absolute stability criterion for the systems with the single hysteresis nonlinearity provides the simplest and pictorial representation of results of the investigation of the stability and the possibility of the synthesis of the correcting devices of the system ensuring the stability of the strain control systems with the electromagnetoelastic actuators. The characteristics of the electromagnetoelastic actuators are the alternating-sign hysteresis type for the piezoactuators and the constant-sign butterfly type for the electrostriction actuators. In the magnetostriction and electrostriction actuators their initial operating point is chosen on one wing of the butterfly, for example, in the first quadrant, for the deformation range to be symmetric at both sides of the initial point. For the butterfly characteristic the initial working point displaced by the half deformation range. The values of the tangents of the inclination angles of the tangent line to the hysteresis nonlinearity on the butterfly wing for the electromagnetoelastic actuator are determined similar to the hysteresis characteristic. The stationary set of the control systems is the segment of the straight line. The absolute stability conditions with the condition on the derivative of the control systems with piezoactuator deformation in the case of the longitudinal, transverse and shift piezoeffect for the hysteresis characteristic of the deformation of the piezoactuator are obtained. The obtained absolute stability conditions for the control system with the electromagnetoelastic actuator allow one to estimate and calculate the characteristics of the control system of the deformation of the electromagnetoelastic actuator.
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