Silage Corn Response to Sulfur in Some Calcareous Soils 
Abstract
Sulfur is a byproduct of gas and oil refineries, that is produced in Iran more than two million tons annually. In this research, the effects of bentonite- sulfur which has been produced with a new process, was tested on corn (SC 704) at Isfahan, Shiraz and Jiroft sites in research farms as a factorial experiment. 0, 0.5, 1 and 2 t ha-1 elemental sulfur and also 0, 65 and 100% recommended phosphorous were applied. The results indicated that sulfur phosphorous and their co-application significantly increased corn shoot dry and wet weight, only in Shiraz site. Zinc and iron uptake in shoots increased in Shiraz and Jiroft sites respectively because of sulfur usage. The highest Fe uptake was observed in 2,000 kg S ha-1. In any site the treatments had on significant effect on shoot phosphorus uptake.
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