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Abstract (300 word limit)
Automobile industry is expected to change significantly in the coming years and decades. A convenient, technically and economically viable and environmentally friendly transportation system for the future needs to be developed. This requires a comparison  between different technical choices  based on best possible designs achievable. 
The role of hydrogen and fuel cells in the future transportation systems is being widely debated. As they are getting  continuously compared with other  possible options, for example with battery vehicles, it is necessary that efficient system concepts for fuel cell based transportation systems are developed. In this paper, we present an approach to increase the efficiencies while using different fuels for transportation applications, by  making use of different types of fuel cells. 
A concept is presented in which a high temperature fuel cell is used as an electricity producing fuel reformer, in this case a Solid Oxide Fuel Cell (SOFC) and low temperature fuel cells onboard for  vehicle propulsion, in this case  Proton Exchange Membrane Fuel Cells (PEMFC). 
A  trigeneration system fed with natural gas and capable of producing electricity, heat, and hydrogen is proposed. Two modes are presented: a Car as Power Plant (CaPP) mode, in which fuel cell electric vehicles (FCEVs) act as energy and water producers while parked; and a pump mode, in which compressed  hydrogen is produced and pumped  to the vehicle’s fuel tank. Different reforming options are presented and compared, a  catalytic reformer (CR), and a solid oxide fuel cell operating as reformer (SOFCR).  Additionally,  the option of integrating  carbon capture and storage (CCS) is also presented. Results indicate that the SOFCR unit significantly reduces the exergy destruction resulting a trigeneration exergy efficiency of around 60%. Additionally, a brief presentation on applying the concept for other types of vehicles also is  presented.
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