TITLE
OPP0SED PISTON CRANKSHAFT LESS AND CONNECTING ROD LESS IC ENGINE.

There are numerous engine developed to increase the efficiency of IC engine but all have some merits and demerits. To improve the efficiency of IC engine we developed opposed piston crankshaft less and connecting rod less engine. In this engine we use different mechanism to increase efficiency of engine. When arc of circle make symmetry it gives a ellipse and this ellipse gives a trajectory points to movement. If we divide this ellipse in three parts of 120 degree it give two curves to trajectory points to movements.
Why new engine.
1. Higher efficiency.
2.  Higher power output.
3.  Less fuel consumption. 
4.  Low weight. 
5.  Less friction. 
6.  Low lubrication consumption.
7. Low cooling consumption.




Merits of this engine
1. Size and weight.
2.  Less friction due higher efficiency due to fewer parts.
3.  Higher power output.
4.  Reduces to two parts only. 
5.  Low lubrication consumption.
6. Low cooling liquid required due to fewer parts
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