The kinetics to convertation of carbon monoxide to carbon dioxide on the surface of mixed nano-catalyst for reduce the vehicles emissions .
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Abstract: In this article, the kinetics of oxidation process of carbon-monoxide on the nano-catalyst surface has been investigated. The investigation  conducted in different flow conditions and temperature, by the range of T=70-350oC, dependence on kinetic  convertation of carbon monoxide to carbon dioxide in the closed system. İt is determined that speed of conversion process increases by 1.30-1.32 times as temperature increases on the surface of catalyst. At low flow rates the conversion of carbon-monooxide to carbon –dioxide runs more rapidly.   

