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Abstract (300 word limit)				
A constructed wetland is an artificial wetland created for the purpose of treating anthropogenic discharge such as municipal or industrial wastewater. It may also be created for land reclamation after mining, refineries, or other ecological disturbances. Constructed wetlands are engineered systems that use natural functions of vegetation to treat different water streams (1). Plants are often thought of as a treatment pathway.  With a plant mono-culture, it is possible to accurately and to model the behavior of a wetland. In additional, a detailed water characterization is necessary to determine explanatory parameters and inventory the constituents in the water (2). In this paper we provide our researches carried out a a laboratory level, concerning the use of some selected plants in order to be used for the remediation of the wastewater resulted from the pharmaceutical industry. The tested specieswere the algae Chlorella vulgaris and the aquatic plants Lemna minor and Spyrogira sp. The algae culture was obtained by successive selection works starting from an identified cell and then all plant species were kept on special selected growth media. The 5 tested solutions used as representing some natural waste waters consisted in NH4NO3, Pb (NO3)2, MgSO4, ZnSO4 and NaCl. The ions which were analyzed concerning their concentration's evolution during a period of 72 hours (starting from 1%) were: Pb, NO3, SO4, Mg, Zn and Cl. The results indicates a better final situation in the case of those 2 aquatic plants, than in the case of using Chlorella.
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