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Abstract 
This study is particularly oriented towards the valorization of a local natural material, in the adsorption reduction of a medical residue (Paracetamol) frequently found in wastewater. The optimization of the treatment required the study of the influence of several parameters namely: the mass of the adsorbent, the initial concentration of the drug, the pH etc. The results obtained showed that paracetamol adsorbs on diatomite at 14.71 mg / g for an initial concentration of 25 mg / l. The pH of the medium and the ionized form of the molecule is at the origin of this difference of adsorption. The results of the temperature effect give a priori exothermic adsorption.
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