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Abstract (300 word limit)
The monthly time step Water Rights Analysis Package Model (WRAP) is one of the components in the Texas Water Availability Model (WAM) system. Sub-monthly time step capabilities to conventional WRAP based on the monthly time step has been added. In this study, focus was given to key variables for simulating sub-monthly time step WRAP as follows: disaggregation of monthly inflow and routing parameters computation. The daily flow pattern method was utilized for disaggregating Brazos River Authority Condensed (BRAC) monthly inflow and routing parameters based on length are computed. The USACE Southwestern Division Reservoir System Simulation Model (SUPER) model daily unregulated (naturalized) flows from 1939 to 1997 were used to develop daily flow patterns for disaggregating BRAC monthly inflows. The mean values of the daily naturalized flow for 1939 to 1997 were used as the flow pattern for 1900 to 1939 and 1998 to 2007. Also, these daily flow patterns were distributed to the other ungaged control points. The lag times at control points of the BRAC dataset were computed based on the distance of the reaches with consideration of the lag time computed using the SUPER daily naturalized flow. The Muskingum routing parameters K were also computed based on the distance of the reaches. The key variable evaluated in this study provides a sufficient level of accuracy for using the model in flood control operations for a multiple-reservoir system. However, further refinements are possible by expending more time and effort to compile more detailed data.
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Fig. 1. The Brazos River Basin, Texas, USA
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