Structural changes and reactions governing reversibility in shape memory alloys	Comment by Swetha Sandala: Already published. Please find the below links for your reference.

 https://www.nanotechnology.scientexconference.com/index.php/conference-program/osman-adiguzel-elazig
https://www.tsijournals.com/articles/thermomechanical-reactions-governing-reversibility-in-shape-memory-alloys.pdf

Adiguzel O
Firat University, Turkey
Abstract
[bookmark: _GoBack]Some materials take place in class of smart materials with adaptive properties and stimulus response to the external changes. Shape memory alloys take place in this group with shape reversibility character and capacity of responding to changes in the environment. These alloys exhibit a peculiar property called shape memory effect, which is characterized by the recoverability of two certain shapes of material at different temperatures. This property is characterized by the recoverability of two certain shapes of material at different temperatures. These alloys possess two unique abilities: the capacity to recover large strains and to generate internal forces during their activation. Shape memory effect is initiated by successive cooling and deformation treatments, and activated thermally on heating and cooling, with which shape of material cycles between original and deformed shapes in reversible way. Therefore, this behavior can be called Thermoelasticity. The basis of this phenomenon is the stimulus-induced phase transformations, thermal and stress induced martensitic transformations, which govern the remarkable changes in internal crystalline structure and properties of the materials. Thermal induced martensitic transformation occurs on cooling, with cooperative movement of atoms in, <110> type directions on the {110} type planes of austenite matrix, along with lattice twinning and ordered parent phase structures turn into twinned martensite structures. The twinned structures turn into detwinned structures by means of stress induced transformation by stressing the material in the martensitic condition. Martensitic transformations are diffusion less transformations, and movements of atoms are confined into neighbor atom distances. 
Shape memory alloys exhibit another property called superelasticity. This behavior is performed in mechanical manner with stressing and releasing the material in elasticity limit at a constant temperature in parent phase region, and shape recovery occurs instantly and simultaneously releasing, by exhibiting elastic material behavior. Superelasticity is performed in non-linear way; stressing and releasing paths are different in the stress-strain diagram, and hysteresis loop refers to energy dissipation. The strain energy is stored after releasing, and these alloys are mainly used as deformation absorbent materials in control of civil structures subjected to seismic events, due to the absorbance of strain energy during any disaster or earthquake.
Copper based alloys exhibit this property in metastable β-phase region. Lattice twinning is not uniform in these alloys and cause to the formation of the complex layered structures with martensitic transformation, like 3R, 9R or 18R depending on the stacking sequences on the close-packed planes of the ordered lattice. 
In the present contribution, x-ray diffraction and Transmission Electron Microscopy (TEM) and Differential Scanning Calorimetry (DSC) studies were carried out on copper based CuZnAl and CuAlMn alloys. X-ray diffractograms taken in a long-time interval show that locations and intensities of diffraction peaks change with the aging time at room temperature, and this result refers to the rearrangement of atoms in diffusive manner.
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