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Abstract
Exposure and radioactivity level of radionuclides in a mineralized zone were investigated on a view to evaluate its radiological health impact in the environment. An advanced Gamma scout survey meter was used to determine the exposure level while a gamma ray spectroscopy (Sodium Iodide detector NaI (TI) determine radionuclides. Some of the radiological indices that were evaluated are the absorbed dose, effective dose, annual equivalent dose, Internal and External hazard indices, annual gonadal dose equivalent, gamma index and the Excess lifetime cancer risk. 
A digital survey meter 992 Fluke Victoreen Gamma Scout Model detector was used to determine the exposure rate in the vicinity of the sampling point. The gamma-scout that was used to determine the exposure level was oriented vertically upward through the survey point. In the whole sampling area, ten different measurements at each site were activities of petroleum drilling, coal mining and bitumen exploration were conducted. The data measured were read directly from the display screen of the gamma-scout. The gamma scout was placed 1 m above the soil level for an hour which enabled us to determine the average exposure in each of the sampling points.
Environmental media (Soil, water and foodstuff) samples were collected in order to determine the radionuclides such as potassium-40, thorium 232 and uranium-238 in the laboratory. All the samples were weighed for the soil (50 g), water (100 ml) and plants (50 g) respectively and put in a well labelled cylindrical airtight plastic container previously washed thoroughly with dilute HNO3 and rinsed with distilled water. Instrumentation analysis was carried out at Centre for Energy and Research Development (CERD), Obafemi Awolowo University, Ile-Ife, Nigeria.
The preliminary results obtained for the exposure level in petroleum drilling environment for ranges from 0.0825 to 0.1134 μSv/hr with a mean value of 0.0945 μSv/hr, while in the bitumen exploration and exploitation area ranges from 0.0870 to 0.1230 μSv/hr with a mean value of 0.1101 μSv/hr and the coal mining environment ranges from 0.075 to 0.1500 μSv/hr with a mean value of 0.1066 μSv/hr respectively. Results obtained were compared to the data obtained by the International Atomic Energy Agency (IAEA), (2000) recommended standard.
The result in this study will provide insight into environmental behaviour and fate of contaminant and serve as baseline data for future investigation and monitoring.
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