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Abstract
The perpetual and interdependent energy and environmental crises caused by fossil fuel consumption should force no one to second-guess renewables, with solar energy among them, as the wave of the future, if not an imperative for our long term survival, along with energy conservation. Perovskite solar cells have been one of the hottest topics as they have shown enormous potential for reaching high power conversion efficiency (PCE), currently above 25% due to very efficient light harvesting, fast charge separation ability, etc. coupled with the low cost of materials and their ease of synthesis/processing from liquid phase. In our work, a novel organic-based interfacial layer was produced in a cost efficient and ecofriendly manner making scalable organics the most promising alternatives to porous inorganic interfaces, which although efficient, struggle with certain limitations. With this novel layer, the perovskite effectively infiltrates into this mesoporous structure, and with enhanced wetting of the surface, the perovskite dramatically increases its homogeneity, thus leading to PCE enhancement and thermal stability [1]. 
	Energy harvesting and energy storage are equal parts of the energy sustainability equation, thus, simple and cheap yet efficient storage must exist as well. In such systems, one of the key aspects of improving overall performance is adequate material selection for electrodes. Mixed transition metal oxides with a spinel structure have been shown to be promising candidates for the design of high-performance pseudocapacitive and battery-type electrodes. The aim of this work was to design a mesoporous structure from liquid phase and subsequent post-processing, with highly conductive carbon fibers and redox-active Co/Mn based mixed oxide spinels [2,3] with highly developed surface area. Electrochemical results in aqueous systems showed high specific capacitance, excellent rate capability and cycling stability. 
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Figure 1: TEM of area around mesoporous interface of perovskite cell, (left); atomic resolution STEM HAADF of nanocrystal noted in center image with atomistic model of Co1.5Mn1.5O4 (right).
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