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Abstract 
[bookmark: _GoBack]Quantum-Dot/Dash (Qdot/dash) chip-scale optical frequency comb(OFC) lasers are promising compact solutions to generate low timing jitter and high spectrum efficient optical pulses for applications in wavelength/freqency-division multiplexing with advanced modulation formats. In this paper, we present semiconductor Qdot/dash C-band single-section passively mode-locking based broadband OFC lasers with mode spacings from 10-90 GHz. The laser active gain material is five-stacked-layer InAs Qdots or Qdashs embedded in InGaAsP waveguide core with the average density of 3.5×1010 cm−2 in each layer. The performances of lasers are investigated in detail. Typically, we acheived the average RIN value as low as - 133.54 dB/Hz and the phase noise less than 1.5 MHz for each filtered individual mode with total 56 channels for a Qdot laser with mode spacing of 28.4 GHz. Moreover, a pulse-to-pulse timing jitter of 2.1 fs and pulse-to-clock timing jitter of 564.8 fs with integrated frequency range from 35 kHz to 20 MHz are obtained. By employing this ultralow noise and timing jitter laser with 56 wavelength channels as optical carriers, 12.5 Terabit/s aggregate data transmission capacity is demonstrated with dual-polarization 16 QAM and base modulation rate of 28 GBd over a 100 km standard single-mode fiber. In addition, using a Qdash double wavlength DFB laser, we successfully demonstrate various real-time broadband optical heterodyne synthesizer based millimeter wave-over-fiber wireless links featuring multi-Gb/s data rates with a maximum data capacity of 36 Gb/s(64-QAM × 6-GBaud) having EVM and BER below the standard 7% overhead FEC limit of 3.8x10-3[3]. These performances are obtained without any form of feedback to control the laser linewidths. These results may lead to an important step towards small size, cost-efficient, low noise, low timing jitter, and a high number of multi-channel light sources for advanced optical and wireless networking systems with upto the capacity of Terabit/s or even higher.
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