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Abstract:
In the recent years heterojounction based photocatalysts are becoming attractive due to the improved catalytic efficiency through delayed charge recombination. However designing and fabrication of such materials are tricky to achieve proper p-n junction interfaces. In this context 2D materials provide better scope in fabricating the proper catalyst due to the available surface for deposition of other semiconductors. Transition metal chalcogenides & MXenes are important new 2D materials which exhibit improved surface properties after exfoliation to 2D structures. We explored the use of both MoS2 and Ti3C2 (MXene) 2D materials after liquid phase exfoliation using different solvents. New tertiary heterostructures were designed by depositing cauliflower-shaped CdS and nanosized Cu2O on exfoliated 2D MoS2 & 2D Ti3C2 via hydrothermal technique. Interestingly doped TiO2 is formed on the surface of Ti3C2 during hydrothermal treatment thus creating a third semiconductor. Materials were characterized by HRTEM, Raman, XPS, SEM and UV-VIS spectroscopy. Water splitting activity was studied in the presence of different organic materials. Lactic acid is found to be most    efficient    with    the    obtained    rate    of    11.5mmol/g/h    and 13.3mmol/g/h     on     MoS2-CdS-Cu2O     and     (TiO2)Ti3C2-CdS-Cu2O, respectively with good repeatability under visible light. Efficient interfacial charge separation is observed from demised photoluminescence intensity which indicates the suppression of hole- electron recombination in the tertiary heterostructure. Mott-Schottky analysis confirms the p-type nature of Cu2O thus facilitating the p-n jounction formation. Substantial increased hydrogen evolution on tertiary materials is discussed based on the proposed mechanism of dual p-n junction based on XPS and Mott-Schottky analysis. Comparatively better efficiency is explained through the high conductivity of Ti3C2. Increased efficiency and stability of the developed noble metal-free catalyst is explained on the basis of synergistic effect of dual p-n junction, improved visible light absorption, formation and enhanced interfacial charge separation on 2D sheet. [1-5]
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Figure 1: Water splitting and electron-hole separation mechanism in dual p-n junctions of the tertiary hetero catalyst.
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