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Abstract
Biodiesel usage, especially in cold climate regions, is very much limited due to the presence of minor components such as steryl glycosides (SG). Therefore, it is crucial to remove SG in order to widen the usage of biodiesel worldwide. For the purpose, various low-cost adsorbents are utilized to remove SG and improve the filterability of biodiesel. Among the adsorbents, activated carbon, silica and beach sand are the promising candidates, mainly due to their surface characteristics with high surface area. The efficiency of these adsorbent is determined by executing the cold soak filtration test.

