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INTERFERENCE FILTERS WITH ABSORPTIVE METAL FILMS 

Metal-dielectric interference filters (IF) offered for technical implementation. Their peculiarity is that the metal films are placed near the interference layer thickness equal to half the wavelength. This design allows to absorption the radiation in the spectrum above the main transmission maximum. An example of the implementation of an IF with a wavelength of 4.3 microns is given.

