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I. Abstract
A series of alloy systems take place in a class of adaptive structural materials called intelligent materials by giving stimulus response to changes in the external conditions. Shape memory alloys take place in this group by exhibiting a peculiar property called shape memory effect, which is characterized by the recoverability of two certain shapes at different temperatures.  These alloys are cooled deformed plastically and recover the original shape after these processes, and cycle between the deformed and original shapes on cooling and heating, respectively. The strain energy is stored with plastic deformation, and released on heating, by means of reverse austenite transformation. These alloys are used as functional materials in many fields from biomedical to the aeronautical industry. In particular, they are used as deformation absorbent materials in control of civil structures subjected to seismic events. Shape memory effect is initiated by successive cooling and deformation processes and performed thermally by heating and cooling, shape of materials cycle between original and deformed shapes in bulk level, whereas the crystal structure cycles between the twinned and ordered parent phase structures, by means of forward martensitic and reverse austenitic transformations. This behaviour is called thermoelasticity. Shape memory effect is governed by two crystallographic transformations, thermal and stress induced martensitic transformations.  Thermal induced transformation occurs along with lattice twinning on cooling and ordered parent phase structures turn into twinned martensite structures. Twinned martensite structures turn into detwinned martensite structures by means of stress induced transformation by deforming plastically in martensitic condition. Thermal induced martensitic transformation is lattice-distorting phase transformation and occurs as martensite variants with the cooperative movement of atoms in <110>-type directions on {110}-type planes of austenite matrix by means of shear-like mechanism. Martensitic transformations occur by two or more lattice invariant shears on {110}-type planes of austenite matrix which is basal plane or stacking plane for martensite.   In the martensitic transformation, the lattice of high temperature austenite phase has greater crystallographic symmetry than that of the low-temperature product phase.  
Copper based alloys exhibit this property in metastable β-phase region, which has bcc-based structures at high temperature parent phase field. Lattice invariant shears are not uniform in copper based shape memory alloys, and the ordered parent phase structures martensitically undergo the non-conventional complex layered structures on cooling.  The long-period layered structures can be described by different unit cells as 3R, 9R or 18R depending on the stacking sequences on the close-packed planes of the ordered lattice.  The unit cell and periodicity is completed through 18 layers in direction z, in case of 18R martensite, and unit cells are not periodic in short range in direction z. In the present contribution, x-ray diffraction and transmission electron microscope studies were carried out on two copper based CuZnAl and CuAlMn alloys. These alloy samples have been heat treated for homogenization in the β-phase fields. X-ray diffraction profiles and electron diffraction patterns reveal that both alloys exhibit super lattice reflections inherited from parent phase due to the displacive character of martensitic transformation. X-ray diffractograms taken in a long time interval show that diffraction angles and intensities of diffraction peaks change with the aging time at room temperature. In particular, some of the successive peak pairs providing a special relation between Miller indices come close each other, and this result refers to the rearrangement of atoms in diffusive manner.
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