

Retinal vascular network based Biomimetic  Microchannel for LOC applications.


[bookmark: _GoBack]Micro channels are identified as an important components that transfer liquids within a minute area for microfluidic applications. The design and simulation of micro channel with a specific volume of fluid using COMSOL Multiphysics. Pressure controlling is an efficient and most accurate way to introduce a certain velocity to component of equipment. In this study, we described the simulation analysis for micro fluidic channels with three inlets and one outlet and went on to optimize it to two inlets and one outlet with appropriate velocity profiles and pressure profiles. The grooves in the micro channel are mimicked from vascular network of the retina which is a dynamically interconnected structure composed of three planar vascular layers with bends and grooves at its tip ends. Different fluids enter the inlets and are supposed to get mixed as much as possible before leaving the outlet. The geometry needs to be modified to increase the mixing of the two fluids within 0.05 sec. There are nine variables that are allowed to change during the geometry optimization. A passive approach to induce mixing of the biological samples is facilitated by increasing the distances. The fluids travel longer distances for mixing because of  inertial and diffusive forces for which the fluids have to travel long before mixing takes place. The channel length is increased by introducing a groove along the center of each channel so as to increase the length for the mixing to happen with the same area as before. Then it is still optimized form three input micro channel to a two input micro channel with appropriate results.

