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I. Abstract 
Carbone dioxide flooding has been applied worldwide as a successful enhanced oil recovery. It may be applied as 
a continuous injection or as water alternating gas (WAG) process. Optimization of the injection mode is important for field application. This paper focuses on using a fully compositional simulation model for “AEB-3C” sandstone oil reservoir; in one of the Western Desert oil fields in Egypt; to predict the impact of CO2 miscible flooding on the reservoir oil recovery and net present value (NPV), to define the best mode of operation that is straight CO2 injection or (WAG) processes and to show the difference between pure and impure CO2. Moreover, several sensitivity runs were done on the oil price to show minimum profitable value of oil price when applying such method in the subject field.

The reservoir under study has been producing under a successful water flooding project since May-2010. The recovery factor by the end of water flooding is predicted as 32%.

CO2 flooding processes have started by the end of water flooding. CO2 is taken from the flared gas (which containing 75% CO2 of its composition) of the nearest gas plant (12 km away).

A significant increase in the oil recovery factor was noticed; it reached up to 57%. Comparisons between different modes of operations were shown which showed better results when applying WAG process than that with straight CO2 injection. Moreover; sensitivities were done on the cycle periods in WAG processes which showed increase in the recovery factor with shortening the cycle periods. In addition to a comparison between pure and impure CO2 which showed very close results.
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