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A b s t r a c t                           
Arsenic and antimony are metalloids, naturally present in the environment but also introduced by human activities. Both elements are toxic and carcinogenic, and their removal from water is of unquestionable importance. Thus, the present research has been conducted for removal of As(III) and Sb(III) from synthetic groundwater by using chemically-modified biomass of marine green algae Posodonia Oceanic (PO-Fe nanocomposite). The PO-Fe nanocomposite was characterized by XRD, FTIR, EA, BET, RMN, SEM, TGA and DTG. Various parameters including contact time, pH, adsorbent dosage, initial concentration and temperature were optimized to achieve maximum adsorption capacity. Adsorption kinetics results of individual and simultaneous arsenic and antimony were analyzed using the pseudo first order, pseudo second order, intra-particles diffusion and the Boyd model. The adsorption isotherm using Langmuir, Frendlich, Temkin, Elovich, Dubinin–Radushkevich (D–R) and Dubinin–Astakhov (D–A) have also been studied. The present adsorption process is able to reduce the As(III) and Sb(III) concentration of synthetic groundwater to below 10 µg/l and 5 µg/l, respectively, which are maximum contaminant level of these elements in drinking water according to WHO guidelines.
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