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Application of Artificial Neural Networks for the prediction of performance of Desiccant Material for Desiccant Cooling System
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Abstract (300 word limit)
Desiccant cooling system (DCS) is an alternate suitable option against conventional cooling system in humid climates. A typical system combines a dehumidifier that uses dry desiccant wheel with desiccant material, with direct or indirect evaporative systems and a sensible cooling system. DCS is the environmental protection technique for cooling purpose of the building. Desiccant wheel is main key component of the DCS and this wheel has desiccant material. The desiccant materials may be a suitable option for better use of evaporative cooling techniques in warm and humid climate. The dehumidification of air by adsorption is a physical process by desiccant materials that attracts the molecules of water present in air on the adsorbent surface. Desiccant materials attract moisture from the air by creating an area of low vapour pressure at the surface of desiccant. Some common adsorbents used are SiO2 (Silica gel), LiCl, Al2O3 (Activated alumina), LiBr and Zeolite. This system reduces the level of chlorofluorocarbons (CFC) in the environment because it restricts the use of conventional refrigerant. An Artificial Neural Network (ANN) was constructed to predict symptoms of desiccant wheel for any climatic conditions. The symptoms of desiccant wheel were outlet specific humidity and outlet dry bulb temperatures. Feed-forward network was employed with resilient back-propagation (trainrp) algorithm used as the training function. The outputs from the network were obtained and validated with the experimental results. Among the constructed networks, the best prediction performance was observed in two-hidden-layered network with minimum error. The modelling of the desiccant wheel was carried out with neural network toolbox of MATLAB® with two inputs (specific humidity and temperature at inlet) and two outputs (specific humidity and temperature at outlet) values. The performance index (Mean square error) for specific humidity and temperature were calculated as 0.00209 and 0.00579 respectively. The proposed model may be used for any climatic conditions to predict the output from the desiccant wheel for the design of the solid desiccant based cooling system in humid climate.
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