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[image: ]Abstract 
Statement of the Problem: Researchers have reported that current wastewater treatments are not efficient in pharmaceuticals removal. Then they are released to environment through wastewater contaminated by the industry and consumers urine or faeces, both human and veterinary. Due to their biological activity, pharmaceuticals are potentially ecotoxic although their effects are not fully understood. Anyway, there is a growing concern on them and new wastewater treatments are studied to improve pharmaceuticals removal in highly contaminated water, as hospital and pharmaceutical industry wastewater effluents. The purpose of this study is to assess biooremediation treatment in terms of removal efficiency and identification of degradation processes. Methodology & Theoretical Orientation: Artificially contaminated water with ten selected pharmaceuticals was used for in vitro experimental treatment with fungus. Controls were defined to identify removal not caused by fungal metabolisation. Pharmaceuticals and their degradation products were analyzed by HPLC-HRMS both in water and fungus. A library of previously reported degradation products was used for the screening. Findings: Trametes versicolor was in average the most efficient fungus for water treatment in this experiment. Each fungus specie studied had considerable differences in removal efficiency of some selected pharmaceuticals and performed degradation by different metabolic pathways. All degradation products detected are reported to be less toxic than the parental pollutant. Some transformation products and parental compounds were detected at the fungal pellet. Conclusion & Significance: Fungi studied were in average as useful to detoxify water with high pharmaceuticals concentration as conventional wastewater treatment. Scaling up and combining the fungi studied should be done to assess performance and synergy between fungi species. Even though, elimination of solid fungal pellet should be studied as some pollutants were adsorbed onto it. 

Image
[bookmark: _GoBack]Figure 1: Representation of total elimination of target pollutants in liquid phase (n=3) and solid phase (n=1) of experimental batches for each fungal treatment. Elimination is calculated as the sum of the ten selected pollutants relative chromatographic peak area (A), referred to the chromatographic peak area detected at initial time (t0) in liquid phase (LP). The peak areas used are expressed as area arbitrary units/mL, both in liquid and solid phase.
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