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Abstract
The orthotropic materials are one of the most important construction elements. In many cases the orthotropic is the relic of technological process like plate rolling. Because the mechanical properties of such type of material depend on the chosen sheet rolling direction, the ability to predict the strength situation is very important, when the material will be destroyed. Very useful can be the strain energy based methods which were used among others in papers [1] and [2]. Sheet rolling direction of sheet metal and mechanical properties changes can be important when loaded part of device is under dynamic impacts. Fatigue processes initiation depends also on local material properties differences and micro notches.
The authors of the presentation applied the strain energy density function for the analytical description of the behaviour of the orthotropic material forced in plane state of stress. The described investigation results are presented on a practical example of the back surface of the thin-walled cylindrical tank under the influence of internal pressure. The material stability assumptions formulated on the basis of the strain energy density function, will be very useful and important in the prediction of failure of material due to a plastic flow and particularity in the assessment of strength of the responsible cylindrical shell. As mentioned, dynamic impacts and fatigue phenomena depend on local material properties and notches shapes. Strain energy based method proposed by authors can be develop and helpful for researchers and engineers interested in the design of the responsible constructions. The proposed energy method is universal and can be modified for the investigated model of construction and applied materials also unconventional materials such as composites or polymers.
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Fig. 1 Orthotropic tank
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