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[bookmark: OLE_LINK4][bookmark: OLE_LINK5]Recent years, layered van der Waals crystals consist of individual atomic planes weakly coupled by vdW interaction have attract great interests due to their intriguing physical properties, such as superconductivity, high carrier mobility, topologically protected surface states and among many others. An ambitious practical goal is to exploit planes of vdW crystals as building blocks of more complex optoelectronic application, especially in the terahertz band. The pursuit of two-dimensional materials for terahertz detection is promoted by the unique properties beyond traditional system, such as good CMOS-compatibility, easy for fabrication and fast response. Especially, graphene can support terahertz plasmon which can lead to enhanced THz absorption. Graphene-based terahertz detectors rely on the photothermoelectric and self-mixing effects[1] both of these effects depends on the near-field or the decay of plasmons. Also, other two-dimensional materials such as black phosphorus, topological insulator exhibit exotic THz optoelectronic properties, such as anisotropic band structure in black phosphorus (BP), interplay between surface states and bulk states such as in Bi2Se3 exhibiting the unique THz spectral profile[2][3]. Initial characterization has demonstrated the excellent interaction between THz photons and two dimensional materials. However, convent absorbed photons into electricity with high efficiency is still a big challenge. In typically, self-mixing process for direct detection require materials with both high mobility and moderated bandgap, and is usually wipe out/disrupted by the coexisting mechanism such as thermoelectric process. In this work, we present a new route toward manipulation of hot electrons within high mobility materials such as BP and graphene. Due their moderated bandgap, the hot electrons in atomic plane can be extensively excited and randomized. The unilateral flow of excess hot electrons can be facilitated by exploring the both the electromagnetic engineering and electrostatic tuning. Intriguingly, the hot electrons effect change the resistance via nonequilitrum carrier diffusion, leading to the high photoelectric gain under electrical bias. The present results and the novel hot electron mechanism allow for realistic exploitation of two-dimensional materials for large area, fast imaging.  
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