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The present investigation has been carried out in the CubaRon S.A. distillery. In this plant technological changes have been made with respect to the original design. Therefore, in this work, a simulated case study has been carried out to determine the best feed plate in the distillation columns. Through the simulation in HYSYS it has been intended to determine the points where to make the injections in the three distillation columns. The new proposal must guarantee that the alcoholic strength is at least 95.5% v / v.

