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Application of the evaporative fraction in estimating daily evapotranspiration based on hourly measurement in water-saving irrigated rice field 
Xiaoyin Liu, PhD, College of agricultural engineering, Hohai University, Nanjing, China
Abstract 
Evaporative fraction (EF), which is known to exhibit variation in response to changes in crop species, soil and meteorologic conditions, plays an important role in interpreting the components of energy budget and estimating evapotranspiration (ET), while such information is scarce for humid rice fields. The present study examines the pattern of hourly, daytime and daily EF after monitoring energy components by eddy covariance for water-saving irrigated (WSI) rice paddies of 2015 and 2016, and estimates the daily ET by an improved EF up-scaling method in the subtropical monsoon climate region of East China. Main results indicate that EF exhibits obviously greater than the reports that from upland crops. Diurnally, hourly EF is deemed as an approximately concave-up shape in different growth stages of rice season. The seasonal average value varies gently, with a minimum around 10:00–11:00 AM. Seasonally, the mean daytime EF for the whole growth stage is 0.86, 7% lower than the daily value. Daily EF exhibits mostly higher than 0.8 except later yellow ripening period, approaching 1.0 in the milk stage. In addition, differences are noted in the results with respect to the daily ET estimation by EF up-scaling method. The estimated daily ET (ETEF,d) from hourly EF during 10:00–11:00 h is highly correlated to the measured ET (ETtrue) by the weighed micro-lysimeters though the ETEF,d value is underestimated. Such a considerable gap serves in forming a relationship between ETEF,d and ETtrue,d, that is, by simply multiplying the representativeness ET value based on the EF up-scaling method by a correction procedure calibrated for this region. In conclusion, an improved EF up-scaling method is proposed for estimating effective daily ET.
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Fig. 1 Behavior of the daily and daytime evaporative fraction (EF) and corresponding precipitation (P) and irrigation (I) during the rice season of (a) 2015 and (b) 2016
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Fig. 2 Behavior of the measured (ETture) and simulated ET (ETEF) (based on 10:00–11:00 period) and corresponding available energy (Rn–G0) during the rice season of (a) 2015 and (b) 2016 (RE, IT, MT, LT, JB, HF, MI and YR represents the re-greening, early tillering, middle tillering, later tillering, jointing and booting, heading to flowering, milk and yellow ripening stage, respectively)
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