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Abstract: Layers of naturally occurring clay minerals are rearranged to prepare highly sensitive multi-responsive clay-clay bilayer membrane (CCBM). The CCBM introduced here responds to the minuscule changes in the surrounding environments including temperature, humidity, and presence of solvent vapors by morphing in specific manners. Inheriting the natural stability of clay minerals CCBM demonstrates extreme robustness, heating up to 500 °C, cooling with liquid N2 and exposure to corrosive chemical vapors did not deteriorate its bending performance. Mechanistic studies suggested that shape transformations of CCBM are driven by the unequal response of its components to external stimuli.

