ABSTRACT
Dealer PDI (Pre-dispatch inspection) report and MQN (market quality news) had given feedback for the water mix in the engine oil of the tractors of all models. This water mixing leads to the loss of value of oil and also affects the life of the engine components working inside the engine assembly. Based on the feedback from the PDI area of the plant, same problems were also being faced in the plant also. Tractors having such problem were taken for investigation and analysis for the problem identification.
[bookmark: _GoBack]To eliminate the rejection/wastage of the engine oil in engine assembly due to mixing of water in all models of tractor which is observed in Re-work and Pre-delivery Inspection Stage in the plant before dispatch. Its average in the last 5 months has been 4475 PPM at present while the target is to achieve is 1000 PPM.

