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ABSTRACT
The extreme rains of court duration are the principal cause of brutal and catastrophic flood that can be produced on a number of small basin on the French Alps 
This study consists on a cartography of extreme values of pluviometric parameters, as a Gradex, rains with a period of 10 years, 100 years and 1000 years , for six steps of time ( 1h, 2h, 3h, 6h, 12h, 24h) ; and Montana parameter on the French Alps where the orographic effect  is big and the estimation of reliable values on unmonitored site using data of environmental stations  need the introduction of morphometric information.
The area study covers a surface of 250 km x450 km and dispose of 65 pluviometric stations of average durations between 30 and 35 years 
This study has been done on two steps , first we have done a presentation of a region by a relief and a climate ; second we have displayed pluviometric systems using ACP method.
The idea based on AURELHY method (Analyzing Using Relief for HYdrometeology ) that consists to intervene the local topography by a linear regression and analyzing by kriging the residue of the regression  has been used for this cartography.
