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Abstract
[bookmark: _Hlk87011359]A series of materials take place in class of advanced smart materials with adaptive properties and   stimulus response to the external changes. Shape memory alloys take place in this group, with the shape reversibility characters and capacity of responding to changes in the environment. These alloys exhibit a peculiar property called shape memory effect, which is characterized by the recoverability of two certain shapes of material at different temperatures. These alloys have dual characteristics called thermoelasticity and superelasticity, from viewpoint of memory behavior. These phenomena are governed by thermomechanical ant thermoresponsive reactions in atomic level.  These transformations are stress induced martensitic transformations. Thermal induced martensite occurs along with crystal twinning in self-accommodating manner on cooling and ordered parent phase structures turn into twinned martensite structures. Stress induced martensitic transformations occur along with crystal or lattice detwinning reaction by stressing material in low temperature condition. Superelasticity is performed by stressing and releasing material at a constant temperature in parent phase region, and shape recovery is performed simultaneously upon releasing the applied stress. Superelasticity exhibits the normal elastic materials, but it is performed in non-linear way; stressing and releasing paths are different in the stress-strain diagram, and hysteresis loop refers to energy dissipation. These alloys are used in building industry, against to the seismic events, due to this property. Thermal induced martensitic transformation   occurs with the cooperative movement of atoms in 110>- type directions on {110}-type planes of austenite matrix, by means of shear-like mechanism. 
Copper based alloys exhibit this property in metastable β-phase region.  Lattice invariant shear is not uniform in copper-based shape memory alloys, and cause to the formation of long-period layered martensitic structures with lattice twinning on cooling. The long-period layered structures can be described by different unit cells as 3R, 9R or 18R depending on the stacking sequences on the close-packed planes of the ordered lattice. The unit cell and periodicity is completed through 18 layers in direction z, in case of 18R martensite, and unit cells are not periodic in short range in direction z.
In the present contribution, electron diffraction and x-ray diffraction studies performed on two copper based CuZnAl and CuAlMn alloys. Electron diffraction patterns and x-ray diffraction profiles show that these alloys exhibit super lattice reflections in martensitic condition. Specimens of these alloys aged at room temperature in martensitic condition, and a series of x-ray diffractions were taken duration aging at room temperature. Reached results show that diffraction angles and peak intensities change with aging time at room temperature. Specially, some of the successive peak pairs providing a special relation between Miller indices come close each other, and this result refers to the rearrangement of atoms in diffusive manner.
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