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Abstract (300 word limit)
[bookmark: _GoBack]Polymer Electrolyte Fuel Cells (PEFC) are expected to be as one of next-generation power supply systems due to its low environmental damage, high efficiency, and availability for dispersed power systems and emergency use. Transport resistance of reactant and product materials such as proton, oxygen and water is the determining factor of its efficiency and therefore it is necessary to analyze the transport phenomena of proton, oxygen and water in PEFC as fast as possible to increase its performance and efficiency. Computational Fluid Dynamics (CFD) based on macroscopic transport equations is often used as a conventional numerical analysis. A Membrane Electrode Assembly (MEA) of PEFC, however, consists of Gas Diffusion Layers (GDL), Micro Porous Layers (MPL), Catalyst Layers (CL), and a Polymer Electrolyte Membrane (PEM), where many nanoscale structures are constructed. In such flow fields, the characteristics of transport phenomena in MEA cannot be analyzed at the macroscopic point of view. Molecular simulation is a powerful tool to analyze these phenomena. In this study these nanoscale transport phenomena are analyzed by large scale Molecular Dynamics (MD) simulations and the relation between the nanoscale structures and the transport phenomena is analyzed in detail (Figure 1). Especially, the transport phenomena of proton in PEM which has highly anisotropic water structures, oxygen permeability, oxygen scattering and proton diffusivity of ionomer in CL, and the transport phenomena of nanoscale water droplet in MPL were simulated.  In the analysis of proton transfer in PEM and ionomer, we considered not only Vehicle mechanism but also Grotthus mechanism and the diffusivity of proton at various water contents was estimated. This information leads to a new design concept of materials for next generation polymer electrolyte fuel cells. 
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Figure 1: Large scale molecular dynamics simulations for the 

transport phenomena in PEFC 


