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Abstract
[bookmark: _GoBack]Statement of the Problem: Day after day, plastics are generating a very high amount of waste every year, not only single-use plastics (SUP) for packaging, but also from several other applications such as automotive, building, construction, energy, sports and leisure, transport, etc. All these materials must now be recycled after their end of life (EOF) to comply with the concept of sustainable development (SD) and circular economy (CE), as well as to reduce their accumulation into landfills or even worse in the oceans. Methodology & Theoretical Orientation: In this work, some statistics on plastics recycling we gathered and analyzed to determine the main areas/applications generating plastics wastes. Then, several options were proposed for specific material recycling, in particular related to different structures/compositions (blends, composites, foams, multilayers, etc.). In all cases, the focus was on mechanical recycling. As a first applications, a two-component wheel was selected, each part being made of 100% recycled polymers. The internal part was made of high density polyethylene (HDPE) from rigid bottles, while the external part was a blend of the same HDPE (good interfacial adhesion/compatibility between both parts) with different concentrations (0-95% wt.) of ground tire rubber (GTR). The compounds were produced via twin-screw extrusion and the parts were produced by compression molding.  Conclusion & Significance: The results showed that after processing conditions optimization (temperature, pressure, time, etc.), a wide of properties (rigidity, elasticity, hardness, impact strength, etc.) can be easily obtained by a simple change of the GTR concentration. This indicates that fully recyclable and sustainable plastics parts can be produced for an applications as presented in Figure 1.  Depending on the original materials used, different looks can be obtained which do not need special processes and additives. These results also open the door for further development using different polymers for the dispersed phase (rubbers/elastomers) and the continuous phase/matrix (thermoplastic resins). 
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Figure 1. Typical examples of wheels based on 100% recycled materials. 
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