ABSTRACT: Bleed off treatment unit abbreviated as BOTU is an essential part of closed loop scrubber system. SOx emission in the air is restricted to 0.1% for maintaining safe environment globally and hence scrubber systems are used in cleaning the exhaust gas of the marine engines and reducing the SOx content percentage. Bleed off treatment unit (BOTU) is used in treatment of bleed off of scrubber water. It separates the water contaminating particles from the bleed off water and removes the sludge. The study of components used and working of the Bleed Off Treatment System was done. The results after functional testing of the Bleed Off Treatment Unit were concluded. For directing this assignment essential learning of exhaust gas cleaning system and fluid mechanics is significant. Subsequently starting writing overview of the related subjects was done. The outcomes dependent upon hypothetical reviews and exploratory outcomes are aggregated in this report.
