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Abstract
The quantification of the amount of absorbed light is essential for understanding laser-material interactions and melt pool dynamics in order to minimize defects in additively manufactured metal components. The geometry of a vapor depression, also known as a keyhole, in melt pools formed during laser melting is closely related to laser absorptivity. This relationship was observed by the state-of-the-art in situ high speed synchrotron x-ray visualization and integrating sphere radiometry. These two techniques create a temporally resolved dataset consisting of keyhole images and the corresponding laser absorptivity. In this work, we developed two pipelines for energy absorption prediction. The one-stage approach adopts Convolutional Neural Networks (ConvNets) to learn feature kernels automatically directly yields an absorption value for each x-ray image using the fully connected layer and regression layer. The two-stage approach first generates semantic image segmentation using ConvNets for keyholes, then extracts the geometric keyhole features and finally applies regression models. Motivation for the second approach is that many artificial intelligence tasks can be solved by carefully designing the right set of features to extract for the task and then feeding these features to a simple machine learning algorithm. This is especially applicable in this case, where we already have a clear understanding of which features are relevant and should be extracted. On the other hand, the main advantage of one-stage approach to the stage-stage approach is that it automatically detects the important features and makes a prediction without any human supervision. We compare the two different absorption prediction pipelines in terms of accuracy, generalizability on unseen materials and model interpretability. This work provides a new pathway for process-control and a real-time monitoring system of laser-based additive manufacturing.
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