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I. Abstract Body 
	For long time, organosilicon thin films has a great interest in many applications that are based on the surface modification. Recently more attention has been focused to the use of organosilicon thin films with embedded metallic nano-sized particles as biocide films [1]. In this study, ZnO Nanoparticles have been deposited with organic films by  plasma discharge in order to elaborate biocide thin films. Tow  deposited methods have been combined in order to elaborate biocide films. Dielectric barrier discharge (DBD) and plasma enhanced chemical vapor deposition (PECVD).   The plasma discharge used is generated by a AC power source with frequency of about  19 kHz using HMDSO as plasma gas and ZnO powder. Bacillus bacteria in Muller Hinton environment has been used in order to exhibit the biocide properties of deposited films. It has been observed that almost all species are eliminated. 
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