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ملخص البحث
تمثل منحنيات تقدم الدقاق علاقة تغير عمق البئر برقم مرحلة الرفع المطابقة وتؤثر هذه المنحنيات على زمن عمليات الرفع والإنزال.

نتيجة لدراسات حقول عديدة في مناطق مختلفة من العالم فقد تم التوصل لعلاقات رياضية تمثل منحنيات تقدم الدقاق قد يكون الشكل العام متشابه وتختلف بثوابتها التجريبية من حقل لأخر.

أوجدنا في هذا البحث العلاقات الرياضية لمنحنيات تقدم الدقاق وحددنا ثوابتها وفق ظروف الحقول السورية وذلك بهدف استخدام هذه المعادلات في:

1. تحديد الطول الكلي للمواسير المرفوعة من البئر عند كل سرعة.

2. حساب الزمن الميكانيكي الأصغري لعمليات رفع المواسير من البئر اعتماداُ على سرع الأجهزة الرافعة ومواصفاتها.

3. تحديد فترة تحميل أجزاء مجموعة الرفع وذلك بهدف حساب فترة استخدامها (مضاجع بكرات ثابتة ومتحركة، كبل الحفر ...) وذلك من اجل التخطيط لعمليات حفر الآبار المستقبلية.
Determination the mathematical equation constants of the Bit penetration curves to guide the trip round
according to Syrian fields' conditions
Dr. Hadid Mahmoud
ABSTRACT

Bit penetration curves indicate the relation between well depth changing and its each trip phase, and also effect the trip round period.

 Mathematical equations have reached as a result of numerous studies in many fields in the world. General structure of these curves maybe the same but the differ in their experiential parameters from one field to another.

In this search, we determined the mathematical equation of the bit penetration curves, and determine their constants according to Syrian fields' conditions, at the aim of: 

· Determining the total length of retrieved pipes at each drawwork velocity.

· Calculating the minimum mechanical time to lift pipes from well based on drawworks velocities and properties.

· Determining period of using the hoisting system (including bearings, both crown and traveling blocks, wire line (drilling cable), desiring to organize future drilling operations.    
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